# omron.v7

Частотный преобразователь Omron V7.

Используемый протокол - MODBUS.

http://www.omronkft.hu/nostree/pdfs/inverter/cimr-v7az/v7az.pdf

    plugin.peripherial:

      module.omron1:
        portnum:  2
        netaddr:  1
        enable:   on
        type:     omron.v7

## Теги

    Reg0001
    Reg0002
    Reg0020
    Reg0021
    Reg0022
    Reg0023
    Reg0024
    Reg0027
    Reg0028
    Reg0029
    Reg002A

    SYSTEM.ErrorCount
    SYSTEM.ErrorFlag
    SYSTEM.NetAddr
    SYSTEM.Port
    SYSTEM.TimePeriod
    SYSTEM.UpdateDate
    SYSTEM.UpdateTime

### Регистры

- Reg0001
  - 0 Run Command - 1: Run, 0: Stop
  - 1 Reverse Run Command 1: Reverse run 0: Forward run
  - 2 External fault 1: Fault (EFO)
  - 3 Fault Reset Command 1: Reset Command
  - 4 Multi-function input reference 1 (Function selected by n050)
  - 5 Multi-function input reference 2 (Function selected by n051)
  - 6 Multi-function input reference 3 (Function selected by n052)
  - 7 Multi-function input reference 4 (Function selected by n053)
  - 8 Multi-function input reference 5 (Function selected by n054)
  - 9 Multi-function input reference 6 (Function selected by n055)
  - A Multi-function input reference 7 (Function selected by n056)
  - B-F (Not used)
- Reg0002 - Frequency reference (unit: n152)
- Reg0020 - Status signal
  - 0 Run Command 1: Run 0: Stop
  - 1 Reverse Run Command 1: Reverse run 0: Forward run
  - 2 Inverter operation ready 1: Ready 0: Not ready
  - 3 Fault 1: Fault
  - 4 Data setting error 1: Error
  - 5 Multi-function output 1 (1: MA ON 0: MA OFF)
  - 6 Multi-function output 2 (1: P1 ON 0: P1 OFF)
  - 7 Multi-function output 3 (1: P2 ON 0: P2 OFF)
  - 8-F (Not used)
- Reg0021 - Fault description
  - 0 Overcurrent (OC)
  - 1 Overvoltage (OV)
  - 2 Inverter overload (OL2)
  - 3 Inverter overheat (OH)
  - 4 (Not used)
  - 5 (Not used)
  - 6 PID feedback loss (FbL)
  - 7 External fault (EF, EFO), Emergency stop (STP)
  - 8 Hardware fault (FXX)
  - 9 Motor overload (OL1)
  - A Overtorque detection (OL3)
  - B Undertorque detection (UL3)
  - C Power loss (UV1)
  - D Control power fault (UV2)
  - E MEMOBUS communications timeover (CE)
  - F Operator connection fault (OPR
- Reg0022 - Data link status
  - 0 Data write in
  - 1 (Not used)
  - 2 (Not used)
  - 3 Upper/lower limit fault
  - 4 Consistency fault
  - 5-F (Not used)
- Reg0023 - Frequency reference (unit: n152)
- Reg0024 - Output frequency (unit: n152)
- Reg0027 - Output current (10/1 A)
- Reg0028 - Output voltage reference (1/1 V)
- Reg0029 - Fault description
  - 0 (Not used)
  - 1 (Not used)
  - 2 Input open phase (PF)
  - 3 Output open phase (LF)
  - 4-F (Not used)
- Reg002A - Alarm description
  - 0 Operation function stop (STP)
  - 1 Sequence error (SER)
  - 2 Simultaneous FWD/REV Run Commands (EF)
  - 3 External Baseblock (BB)
  - 4 Overtorque detection (OL3)
  - 5 Cooling fan overheat (OH)
  - 6 Main circuit overvoltage (OV)
  - 7 Main circuit undervoltage (UV)
  - 8 Cooling fan fault (FAN)
  - 9 Communications fault (CE)
  - A Option card communications error (BUS)
  - B Undertorque (UL3)
  - C Inverter overheat alert (OH3)
  - D PID feedback loss (FBL)
  - E Emergency stop (STP)
  - F Communications waiting (CAL)